***Tilt & Retractable Blinds***:

**Type 80a6**

80x0.44mm external aluminium venetian blind, with rolled edge slats, sound deadening slat inserts and extruded guide rails.

Max Width - 6000mm Max Height - 5000mm

Min Width - 700mm Min Height - 1000mm

Limited to a Max Area - 18m2

**Type 80a2**

80x0.44mm external aluminium venetian blind, with rolled edge slats, sound deadening slat inserts and tensioned guide wires.

Max Width - 6000mm Max Height - 5000mm

Min Width - 700mm Min Height - 1000mm

Limited to a Max Area - 18m2

**Type 80af**

80x0.44mm external aluminium venetian blind, with 'flat' edge slats and tensioned guide wires.

Max Width - 5000mm Max Height - 5000mm

Min Width - 700mm Min Height - 1000mm

Limited to a Max Area - 18m2

**Type 50a**

50x0.21mm external aluminium venetian blind, with 'flat' edge slats and tensioned guide wires.

Max Width - 3000mm Max Height - 3000mm

Min Width - 700mm Min Height - 1000mm

Limited to a Max Area - 9m2

***Tilt Only (non-retractable) Blinds***:

**Type R80**

80x0.44mm external aluminium 'tilt only' blind, with rolled edge slats.

Max Width - 5000mm Max Height - 5000mm

Min Width - 1000mm Min Height - 500mm

Limited to a Max Area - 20m2

**Type R88**

88x1.2mm external aluminium 'tilt only' blind, with extruded slats.

Max Width - 5000mm Max Height - 5000mm

Min Width - 1000mm Min Height - 500mm

Limited to a Max Area - 20m2